This page needs filled out and signed by your mechanic if you are participating in **TRACK DRIVING EXPERIENCE only**. It will be collected at the track. **Snell 2005 helmets or newer required.**

**MBCA PRE-EVENT TECH INSPECTION SHEET**

You MUST bring this completed inspection sheet with you for the track grid inspection.

**You are responsible for the condition and repair of your vehicle. MBCA’s acceptance of this inspection sheet affords no guaranty or warranty to anyone regarding condition, repair, defects or failure of performance of the vehicle.**

Name\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Year\_\_\_\_\_\_ Car Model\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Lic. Plate #\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Mileage\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

ENGINE COMPARTMENT ok fail REAR SUSPENSION ok fail

Accelerator linkage/bushings/ \_\_ \_\_ Axle shafts/boots \_\_ \_\_

springs

Air filter bracket, mounting \_\_ \_\_ Shocks/leakage/rubber bushings \_\_ \_\_

Battery frame/hold-down \_\_ \_\_ Springs/center spring \_\_ \_\_

Battery/cables \_\_ \_\_ Stabilizer/bushings \_\_ \_\_

Engine clean \_\_ \_\_ Subframe/mounts \_\_ \_\_

Engine mounts \_\_ \_\_ Tire wear-not less than 3/32” \_\_ \_\_

Engine oil/fuel leaks \_\_ \_\_ Trailing arm bushings \_\_ \_\_

Belts \_\_ \_\_

Visco clutch \_\_ \_\_ DRIVE TRAIN

Water pump/water hoses/clamps \_\_ \_\_ Center Support \_\_ \_\_

Water leak \_\_ \_\_ Flex disc/universal joint \_\_ \_\_

Transmission mount \_\_ \_\_

FRONT SUSPENSION

Ball joints/bushings \_\_ \_\_ BRAKES

Draglink/tie-rods \_\_ \_\_ Brake booster \_\_ \_\_

Idler arm bushings \_\_ \_\_ Brake calipers/cylinders \_\_ \_\_

King pins-no play \_\_ \_\_ Brake discs/drums \_\_ \_\_

Shocks \_\_ \_\_ Brake fluid renewed \_\_ \_\_

Springs-No spring spacers \_\_ \_\_ Brake hoses/brake lines \_\_ \_\_

Stabilizer bushings \_\_ \_\_ Master brake cylinder \_\_ \_\_

Steering box, lines, leaks, play \_\_ \_\_ Brake pads/shoes-min. 50% for

Steering shock/coupling \_\_ \_\_ 1 driver; 80% for 2drivers \_\_ \_\_

Subframe Mounts \_\_ \_\_ Brake dust shields removed \_\_ \_\_

Tire wear-not less than 3/32” \_\_ \_\_

Tires-no cuts, bruises \_\_ \_\_ EXHAUST SYSTEM

Wheels-bearing play/damage/ Exhaust leaks \_\_ \_\_

 Bent/correct lugs \_\_ \_\_ Exhaust system secure \_\_ \_\_

OIL LEAKS UNDER CAR

Engine/transmission \_\_ \_\_ LIGHTS/SEAT BELTS/WINDOWS

Rear end/differential \_\_ \_\_ Signals/stoplights/headlights \_\_ \_\_

 Seatbelts/windows-operation \_\_ \_\_

**Note: Use manufacturers recommended brake fluid. Brake fluid must be renewed within 6 months, (but recommended 3 months) of the driving event. Rule 3.4.4-C (brakes)**

NOTE: A road test is recommended on older cars.

Date brake fluid was renewed:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date of inspection:\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Inspection was performed at (Repair shop) Technician’s signature

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

For official use only car #\_\_\_\_\_\_\_ Snell M, SA, or Snell **2005** or newer Safety Helmet\_\_\_\_\_\_\_\_